The following hand signals for rail operations shall be used in accordance with the *Canadian Rail Operating Rules*:

|  |  |  |
| --- | --- | --- |
| **MANNER OF USING** | **INDICATION** |  |
| Swung from side to side at right angle to the track. | STOP |  |
| Swung in a circle at right angle to the track at a speed in proportion to the speed required. | MOVE BACKWARD |  |
| Raised and lowered at a speed in proportion to the speed required. | MOVE FORWARD |  |
| Raised and swung horizontally above the head, at right angle to the track when standing. | APPLY AIR BRAKES |  |
| Raised and held at arm’s length above the head when standing. | RELEASE AIR BRAKES |  |
| Held horizontally at arm’s length. | REDUCE SPEED |  |
| Any object waved violently by anyone on or near the track is a signal to stop. | STOP |  |